For 1990-2009 cars

### Removal Procedure

1. Remove the front seat outer trim cover. Refer to Seat Cushion Outer Trim Panel Replacement.

Important: While carrying out the following procedure, take care not to damage the sill panel trim (1).

2. Carefully disengage the front sill panel trim (1) from the sill (2).
3. Remove the front sill panel trim (1).

### Installation Procedure

1. Install the front sill trim panel (1) to the sill (2).
2. Remove the front seat outer trim cover. Refer to Seat Cushion Outer Trim Panel Replacement.