For 1990-2009 cars

### Removal Procedure

#### Type A

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
3. Carefully pry the front bumper fascia lower grille retaining tabs (1) from the front bumper fascia.
4. Remove the front bumper fascia lower grille from the front bumper fascia.

### Removal Procedure

#### Type B

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
3. Carefully pry the front bumper fascia lower grille retaining tabs (1) from the front bumper fascia.
4. Remove the front bumper fascia lower grille from the front bumper fascia.

### Installation Procedure

#### Type A

1. Install the front bumper fascia lower grille to the front bumper fascia.
2. Firmly press the front bumper fascia lower grille retaining tabs (1) into the front bumper fascia.
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement.
4. Lower the vehicle.

### Installation Procedure

#### Type B

1. Install the front bumper fascia lower grille to the front bumper fascia.
2. Firmly press the front bumper fascia lower grille retaining tabs (1) into the front bumper fascia.
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement.
4. Lower the vehicle.