For 1990-2009 cars

### Window Motor Programming and Setup

If the battery has been disconnected, recharged or replaced, it will be necessary to reprogram each power window for the express-up and express-down feature.

To program each front window, follow these steps:

1. With the ignition in ACCESSORY, RUN, or in the retained accessory power (RAP) mode.
2. Close all doors.
3. Press and hold the power window switch until the window is fully open and continue holding the switch up for approximately two seconds after the window is completely open.
4. Pull the power window switch up until the window is fully closed and continue holding the switch up for approximately 2 seconds after the window is completely closed.

The window is now reprogrammed. Repeat the process for the remaining windows.