For 1990-2009 cars

### Removal Procedure

Important: When a suitable hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

1. Install a suitable hood brace to the vehicle.

Caution: Refer to Safety Glasses Caution in the Preface section.

2. Using a suitable tool, carefully work the hood front seal (1) off the hood from side to side.
3. Remove the hood front seal (1) from the hood.

### Installation Procedure

1. Position the hood front seal (1) to the hood.
2. Install the push-in retainers to secure the hood front seal (1) to the hood.
3. Remove the suitable hood brace from the vehicle.