For 1990-2009 cars

Important: All transmitters which are to be recognized by the remote function actuator (RFA) must be programmed in a single programming sequence. If the system is placed in program mode it will erase all previously programmed transmitters upon the receipt of the programming signal from the first transmitter. Up to 4 transmitters can be programmed. Do not operate or program the transmitters in the vicinity of other vehicles that are in the keyless entry program mode. This prevents the programming of the transmitters to the incorrect vehicle.

1. Install a scan tool.

Important: When the RFA is programmed the remote key and TPMS sensor data will be erased.

2. Use the scan tool in order to access programming: Body/RFA (Remote Function Actuator)/Programming and select either of the following options:

• | Erase all and program remotes.

• | Add additional remotes.

3. Follow the scan tool on screen instructions.

Important: The scan tool must stay connected until all of the transmitters are programmed.

4. Press and hold the LOCK button and the UNLOCK button simultaneously on one transmitter. After a delay of 5-10 seconds, the scan tool will indicate that the transmitter is programmed.
5. Repeat the previous step in order to program up to 4 transmitters.
6. Remove the scan tool.
7. Operate the transmitter functions in within the specified range in order to verify correct system operation.
8. Do not cycle ignition. Final key fob may need to be programmed.