LOOSE/WAVY INSTRUMENT PANEL TRIM PLATE R&R. GMC Truck Caballero 1981

For 1990-2009 cars

# LOOSE/WAVY INSTRUMENT PANEL TRIM PLATE R&R

SOME EARLY 1981 MALIBUS, MONTE CARLOS, & EL CAMINOS MAY EXHIBIT A LOOSE, POOR FITTING OR WAVY INSTRUMENT PANEL TRIM PLATE. THE ATTACHMENT OF THE PLATE TO THE I/P WILL BE REVISED INTERIM 1981. THE FOLLOWING PROCEDURE SHOULD BE FOLLOWED WHEN REPLACING THIS COMPONENT: 1.PROCURE NEW TRIM PLATE (REFERENCE CHART ON PAGE 2). REMOVE TWO (2) UPPER TABS TO RIGHT OF VENTILATION DUCTS, AS ILLUSTRATED ON PAGE 2. 2.REMOVE LOGO (EMBLEM) FROM ORIGINAL TRIM PLATE AND INSTALL ON REPLACEMENT (ATTACHING PUSH-NUT IS P/N 1479948). 3.INSTALL TRIM PLATE TO I/P, LEFT SIDE FIRST, SO THAT PLATE "SNAPS IN" ALONG UPPER & LOWER EDGES. 4.RIGHT SIDE RETENTION CAN BE IMPROVED, IF NECESSARY, BY ADDING TWO (2) 4.2 - 1.41 X 8 MM PAN HEAD CROSS RECESS TAPPING SCREWS (P/N 11501234 OR 9427302) AS ILLUSTRATED, TO INCREASE INTERFERENCE. DEFLECTOR MUST BE FREE TO ROTATE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.