Diagnostic Trouble Code (DTC) List. Geo Prizm 1997

For 1990-2009 cars

DTC | Description | Type | Illuminate MIL
--- | --- | --- | ---
P0105 | Manifold Absolute Pressure (MAP) Sensor Circuit | A | Yes
P0106 | Manifold Absolute Pressure (MAP) System Performance | B | Yes
P0110 | Intake Air Temperature (IAT) Sensor Circuit | A | Yes
P0115 | Engine Coolant Temperature (ECT) Sensor Circuit | A | Yes
P0116 | Engine Coolant Temperature (ECT) Circuit Performance | B | Yes
P0120 | Throttle Position (TP) Sensor Circuit | A | Yes
P0121 | Throttle Position (TP) Sensor System Performance | B | Yes
P0125 | Excess Time To Closed Loop Fuel Control | A | Yes
P0130 | Oxygen Sensor (O2S) Circuit Sensor 1 | B | Yes
P0133 | Oxygen Sensor (O2S) Slow Response Sensor 1 | B | Yes
P0136 | Heated Oxygen Sensor (HO2S) Circuit Sensor 2 | B | Yes
P0141 | Heated Oxygen Sensor (HO2S) Heater Circuit Sensor 2 | B | Yes
P0171 | Fuel Trim System Lean | B | Yes
P0172 | Fuel Trim System Rich | B | Yes
P0300 | Engine Misfire Detected | B | Yes
P0301 | Cylinder 1 Misfire Detected | B | Yes
P0302 | Cylinder 2 Misfire Detected | B | Yes
P0303 | Cylinder 3 Misfire Detected | B | Yes
P0304 | Cylinder 4 Misfire Detected | B | Yes
P0335 | Crankshaft Position (CKP) Sensor Circuit | B | Yes
P0336 | Crankshaft Position (CKP) Sensor Performance | B | Yes
P0340 | Camshaft Position (CMP) Sensor Circuit | A | Yes
P0401 | Exhaust Gas Recirculation (EGR) Insufficient Flow | B | Yes
P0402 | Exhaust Gas Recirculation (EGR) Excessive Flow | B | Yes
P0420 | Three Way Catalyst (TWC) System Low Efficiency | B | Yes
P0500 | Vehicle Speed Sensor (VSS) Circuit -- 4spd. A/T | A | Yes
P0500 | Vehicle Speed Sensor (VSS) Circuit -- M/T and 3spd. A/T | B | Yes
P0505 | Idle Control System | A | Yes
P1300 | Ignition Control Module Circuit | A | Yes
P1335 | Crankshaft Position (CKP) Sensor Circuit | A | Yes
P1520 | Stop Lamp Switch Circuit | B | Yes
P1600 | Control Module Long Term Memory Reset | A | Yes