Fastener Tightening Specifications. Geo Prizm 1996

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 23 N·m | 17 lb ft
Clutch Line Bracket Bolts | 12 N·m | 106 lb in
Clutch Release Cylinder Bolts | 12 N·m | 106 lb in
Clutch Release Lever Bolt and Nut | 23 N·m | 17 lb ft
Extension Rod Retaining Nut | 40 N·m | 29 lb ft
Flywheel Cover Bolts | 20 N·m | 15 lb ft
Front Transaxle Bolt | 60 N·m | 44 lb ft
Gearshift Control Lever Guide Plate Bolts | 10 N·m | 89 lb in
Gearshift Control Lever Housing Nuts | 6 N·m | 53 lb in
Gearshift Control Lever Housing-to-Guide Plate Nuts | 40 N·m | 29 lb ft
Gearshift Guide Case Bolts | 12 N·m | 106 lb in
Gearshift Interlock Bolt | 28 N·m | 21 lb ft
Gearshift Yoke Bolt | 28 N·m | 21 lb ft
Heat Insulator Bolts and Nut | 20 N·m | 15 lb ft
Hold Down Bracket Bolt and Nut | 12 N·m | 106 lb in
Left Case Cover Bolts | 12 N·m | 106 lb in
Left Transaxle Mount Bracket Bolts | 60 N·m | 44 lb ft
Left Transaxle Mount Bolts | 60 N·m | 44 lb ft
Left Transaxle Mount Retaining Nuts | 60 N·m | 44 lb ft
Left Transaxle Mount Through Bolt | 60 N·m | 44 lb ft
Lower Transmission to Engine Bolts

- #1 Bolts

23 N·m

11 lb ft

- #2 Bolts

46 N·m

34 lb ft

Rear Transaxle Mount Retaining Bolts | 60 N·m | 44 lb ft
Rear 3 Mount Nuts | 57 N·m | 42 lb ft
Rear Transaxle Mount Through Bolt and Nut | 60 N·m | 44 lb ft
Right Case-to-Engine Block Mounting Bolts | 60 N·m | 44 lb ft
Speedometer Driven Gear Case Retaining Bolt | 7 N·m | 62 lb in
Starter Bolts | 39 N·m | 29 lb ft
Starter Motor Retaining Bolts | 28 N·m | 21 lb ft
Transaxle Drain Plug | 21 N·m | 15 lb ft
Transaxle Hanger Bolt | 12 N·m | 106 lb in
Transaxle Oil Level/Filler Plug | 21 N·m | 15 lb ft
Transaxle Side Cover Bolts | 12 N·m | 106 lb in
Transaxle Upper Side Mounting Bolts | 64 N·m | 47 lb ft
Vehicle Speed Sensor Bolt | 6 N·m | 53 lb in