SMU - SECTION 6E3 - DRIVEABILITY AND EMISSIONS. Geo Prizm 1994

For 1990-2009 cars

# SMU - SECTION 6E3 - DRIVEABILITY AND EMISSIONS

#### SUBJECT: SERVICE MANUAL UPDATE-SECTION 6E3-DRIVEABILITY AND EMISSIONS- THROTTLE POSITION SENSOR SPECIFICATIONS

#### MODELS: 1993-1995 GEO PRIZM WITH 1.8L ENGINE (VIN 8 - RPO LV6) AND WITH 1.6L ENGINE (VIN 6 - RPO L01)

THE FOLLOWING IS AN UPDATE TO THE TP SENSOR RESISTANCE SPECIFICATIONS, 1993-95 IN SECTION 6E3-C1-9.

________________________________________________________________ | CLEARANCE BETWEEN | BETWEEN TERMINALS | RESISTANCE | | LEVER AND STOP SCREW | | | |______________________|_____________________|_________________| | 0 MM (0 IN.) | VTA - E2 | 0.2 - 5.7 K OHM | |______________________|_____________________|_________________| | 0.40 MM (0.016 IN.) | IDL - E2 | 2.3 K OHM OR | |______________________|_____________________|_LESS_________ __| | 0.90 MM (0.035 IN.) | IDL - E2 | INFINITY | |______________________|_____________________|_________________| | THROTTLE VALVE FULLY | VTA - E2 | 2.0-10.2 K OHM | | OPEN | | | |______________________|_____________________|_________________| | - | VC - E2 | 2.5-5.9 K OHM | |______________________|_____________________|_________________|

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.