Transmission Mount Replacement - Left Side. Geo Prizm 1996

For 1990-2009 cars

#### Tools Required

J 28467-A Universal Support Fixture

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Remove the positive and the negative battery cable.
2. Remove the battery hold down bracket bolt and nut.
3. Remove the battery bracket.
4. Remove the battery and the battery tray.
5. Disconnect the IAT connector.
6. Remove the IAT sensor.
7. Remove the air cleaner hose and cap assembly.
8. Remove the air filter.
9. Remove the 3 air cleaner lower box bolts.
10. Remove the air cleaner box.
11. Support the engine with the J 28467-A .
12. Remove the transaxle left mount through bolt.
13. Remove the 4 bolts and the left transaxle mount.
14. Remove the 3 left transaxle bracket bolts and bracket.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the 3 left transaxle bracket and bolts.

Tighten
Tighten the transaxle bracket bolts to 60 N·m (44 lb ft).

2. Install the left transaxle mount and the 4 bolts.

Tighten
Tighten the left transaxle mount bolts to 60 N·m (44 lb ft).

3. Install the transaxle mount through bolt.

Tighten
Tighten the transaxle mount through bolt to 60 N·m (44 lb ft).

4. Remove the engine support fixture.
5. Install the air cleaner box.
6. Install the 3 air cleaner box bolts.
7. Install the air filter.
8. Install the air cleaner hose and cap assembly.
9. Install the IAT sensor.
10. Connect the IAT connector.
11. Install the battery tray and battery. Refer to Battery Replacement in Engine Electrical.
12. Install the hold down bracket.
13. Install the hold down bracket bolt and nut.

Tighten
Tighten the hold down bracket bolt and nut to 12 N·m (106 lb in).

14. Install the positive and negative battery cables.