Exhaust Gas Recirculation Back Pressure Sensor Replacement. Geo Prizm 1996

For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable.
2. Remove the four vacuum hoses from the EGR pressure transducer.
3. Remove the EGR pressure transducer from the retainer.

### Installation Procedure

1. Install the EGR pressure transducer (1) to retainer.
2. Install the four vacuum hoses to the EGR pressure transducer.
3. Install the negative battery cable.

Tighten
Tighten the negative battery cable-to-negative battery terminal retainer to 15 N·m (11 lb in).