FRONT LICENSE PLATE INSTALLATION. Geo Prizm 1989

For 1990-2009 cars

# FRONT LICENSE PLATE INSTALLATION

#### Model and Year: 1989-90 S CAR

#### TO: ALL CHEVROLET DEALERS

This bulletin provides Dealer Technicians the procedure for installing the front license plate on 1989/90 GEO Prizms.

Because many states do not require front license plates, 1989/90 GEO Prizms which arrive at your dealership will not be equipped with a front license plate mounting provision. Front license plates can be installed, however, by drilling a 15/32 hole into each of the 2 dimples in the front fascia. After drilling, insert a standard license plate nut into each of the holes and attach the license plate with two screws.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.