SMU - SECTION 7A - THROTTLE VALVE CABLE ADJUSTMENT. Geo Prizm 1993

For 1990-2009 cars

# SMU - SECTION 7A - THROTTLE VALVE CABLE ADJUSTMENT

THIS BULLETIN IS BEING REVISED TO INFORM "GM OF CANADA" AND "NAES" DEALERS THAT THEY ARE NOT AUTHORIZED TO UTILIZE THIS SERVICE BULLETIN

*********************************************************************

"GM OF CANADA" AND "NAES" DEALERS ARE NOT AUTHORIZED TO UTILIZE THIS SERVICE BULLETIN.

*********************************************************************

********************************************************************** SERVICE MANUAL UPDATE **********************************************************************

#### SUBJECT: SECTION 7A - THROTTLE VALVE CABLE ADJUSTMENT

#### MODELS: 1993 GEO PRIZM

THE INFORMATION CONTAINED IN THIS BULLETIN AMENDS STEP TWO ON PAGE 7A-28 UNDER "TV CABLE ADJUSTMENT" IN THE 1993 GEO PRIZM SERVICE MANUAL (ST373-93).

2. THROTTLE VALVE POSITION MAKING SURE THAT IT IS FULLY CLOSED (A245E) OR AT WIDE OPEN THROTTLE (A131L).

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.