Throttle Opener Replacement. Geo Prizm 1996

For 1990-2009 cars

### Removal Procedure

1. Remove the throttle body from the intake manifold.
2. Remove the two screws and the throttle opener from the throttle body. Refer to Throttle Body Replacement.

### Installation Procedure

1. Install the throttle opener to the throttle body.
2. Secure the throttle opener with the two screws.
3. Install the throttle body to the intake manifold. Refer to Throttle Body Replacement.