SERVICE MANUAL UPDATE - SEC. 3A WHEEL ALIGNMENT. Geo Prizm 1993

For 1990-2009 cars

# SERVICE MANUAL UPDATE - SEC. 3A WHEEL ALIGNMENT

#### Subject: WHEEL ALIGNMENT

#### Model and Year: 1993 GEO PRIZM

The specifications contained in this service bulletin replace those found in Wheel Alignment (Section 3A) of the 1993 Geo Prizm Service Manual (ST373-93). Use the specifications in this bulletin whenever it becomes necessary to adjust the front and rear wheel alignment.

Front Caster 1.33 Deg. +- 0.75 Deg. Front Cross Caster (Max.) 0.5 Deg. Front Camber -0.17 Deg. +- 0.75 Deg. Front Cross Camber (Max.) 0.5 Deg. Front Total Toe 0.1 Deg. +- 0.2 Deg. Rear Camber -0.92 Deg. +- 0.75 Deg. Rear Cross Camber (Max.) 0.5 Deg. Rear Total Toe 0.3 Deg. +- 0.1 Deg. Steering Axis Inclination 12.58 Deg. +- 0.75 Deg.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.