SERVICE MANUAL UPDATE SEC. 4D DRIVE AXLE TORQUE SPEC CHANGE. Geo Prizm 1991

For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 4D DRIVE AXLE TORQUE SPEC CHANGE

#### Subject: DRIVE AXLE SHAFT HUB NUT AND WASHER CHANGED

#### Model and Year: 1991 GEO PRIZM

The drive axle shaft hub nut and washer design has been changed. A washer based nut is now used to secure the drive axle to the hub. Accordingly, the torque specification has been increased.

#### Tighten

- Drive axle shaft hub nut to 226 N.m (1 67 lbs. ft.).

Please note your copy of the Service Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.