LTG REQUEST FOR REVIEW CHANGES SEPT./NOV. - ALL MODELS. Geo Spectrum 1988

For 1990-2009 cars

# LTG REQUEST FOR REVIEW CHANGES SEPT./NOV. - ALL MODELS

#### Model and Year: ALL MODELS

This bulletin provides updates to the published Chevrolet Labor Time Guide. September through November updates are attached.

These updates will be included in future revisions of the Labor Time Guide, and at that time it is recommended that you dispose of the paper copy.

In the case of past model year updates, it is recommended that a copy of the update be retained with the appropriate model year labor time guide as a complete revision will not be provided.

#### REQUEST FOR REVIEW - PASSENGER CAR

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G J T Y --------------------- NUMBER VIN CODE ------ W LNU P Z CDEF B Y ------------------------- EXTENSION, FRONT FENDER

COLOR COAT .5 NOTE: Applicable model RIGHT A0500 GB years: 1986-1987 .5 LEFT A0501 GB

EXTENSION, FRONT FENDER - REPLACE

#### NOTE: Applicable model RIGHT B1820 .9 years: 1986-1987 .9 LEFT B1821 ADD: .3 A- To Color Coat .............. GB

BRACKET, POWER STEERING PUMP E9020 .6 ASSEMBLY, MOUNTING - REPLACE

#### NOTE: Applicable model years: 1987-1988 with 2.8L V-6.

#### ADD:

A- With A/C .................... .1 B- To Replace Front Mounting Bracket ............ .2

SEAL(S), CRANKSHAFT REAR MAIN - REPLACE J1120 3.5

#### NOTE: Applicable model years: 1981-87 w/auto trans (Chevette)

#### ADD:

A- With P/S ............... .1

TENSIONER, SERPENTINE BELT - REPLACE J0680

#### NOTE: Applicable model years: 1987-88 (Correction to the misprint in the MAY/JUNE Bulletin.) L-4 .7 V-6 .2

ADAPTER AND/OR GASKET, OIL FILTER - REPLACE J0960 NOTE: Applicable model years: .5 1987-88 w/ 2.8L

RELAY, MASS AIR FLOW SENSOR - REPLACE J4650 NOTE: Applicable model years: 1986-88

#### ADD:

A- To Replace Both Relays (V-8 Only) ..................... .1 .1

BOWL, CARBURETOR FLOAT - REPLACE J5100 2.4 NOTE: Applicable model years: 1982-88

#### ADD:

A- With A/C ................... .1

SWITCH - REPLACE ENGINE OIL PRESSURE N2220 .4 NOTE: Applicable model years: All w/ V-6 and gage option (Correction to the JANUARY/FEBRUARY Bulletin.)

#### ADD:

A- With A/C ................. 1.1

INSTRUMENT PANEL CLUSTER COMPONENTS (DIGITAL/ELECTRONIC) - REPLACE ILLUMINATING LAMP N4184 1.1 NOTE: Applicable model years: 1986-1988

TRANSPORTATION CLAIM OPERATIONS LOOSE SHIPPED ITEMS - REPLACE S0014 .2 .2 .2 .2 .2 .2

#### NOTE: Applicable model year: ALL

#### REQUEST FOR REVIEW - PASSENGER CAR

VEHICLE SERIES OPERATION DESCRIPTION OPERATION L M R S --------------------- NUMBER VIN CODE ------ TV RS FG K ----------------

LINK OR SPRING, FRONT DOOR HOLD OPEN - REPLACE NOTE: Applicable model years: 1987-1988 RIGHT B4050 .6 LEFT B4051 .6

WHEELS NOTE: Applicable model years: 1987-1988 COLOR COAT RIGHT FRONT A3300 .4 GB LEFT FRONT A3301 .4 GB RIGHT REAR A3320 .4 GB LEFT REAR A3321 .4 GB SPARE A3340 .4 GB

#### ADD:

A- W/Clear Coat Paint ............. .2 CA

VALVE, VACUUM DELAY - REPLACE J6080 .2 NOTE: Applicable model years: 1985-88

SENSOR, THROTTLE POSITION - REPLACE J6374 1.0 NOTE: Applicable model years: 1985-88 -

CABLE AND/OR 'O' RING, THROTTLE VALVE K6200 1.4 CONTROL (T.V.) - REPLACE NOTE: Applicable model year: ALL

CONVERTER, EXHAUST CATALYTIC - REPLACE L2300 1.2 NOTE: Applicable model years: All

LENS AND/OR GASKET, LAMP - REPLACE NOTE: Applicable model years: 1987-88

REAR COMBINATION RIGHT N1224 .5 LEFT N1225 .5

HORN ASSEMBLY - REPLACE N0200 .4 NOTE: Applicable model years: All

BULBS, LAMP - REPLACE UPSHIFT INDICATOR N0815 .3 .3

BULBS, LAMP - REPLACE NOTE: Applicable model years: 1987-1988

FLASHER - REPLACE HAZARD WARNING N1750 .2 NOTE: Applicable model year: 1987-1988

SWITCH - REPLACE UPSHIFT 1-2 N2361 .3 .3

UPSHIFT 3-4 N2362 .3 .3

#### NOTE: Applicable model years: 1987-1988

CONTAINER AND COVER, WASHER - REPLACE WINDSHIELD N3700 .3

INC: Radiator coolant reservoir. NOTE: Applicable model years: All

HEATER, ENGINE BLOCK - REPLACE R4600 .5 NOTE: Applicable model years: 1987-1988 Add appropriate labor operation time(s) for removal of necessary components to gain access to engine block heater to regular labor hours column.

FRONT DOOR HINGE PIN BREAKAGE T1243 1.7 NOTE: Chevrolet Technical Service Bulletin 88-32, 1987-88 Beretta, Corsica.

#### ADD:

A- To Refinish ......................... .3 GB

TRANSPORTATION CLAIM OPERATIONS NOTE: Applicable model years: All

LOOSE SHIPPED ITEMS - REPLACE S0014 .2 .2 .2 .2

NEW VEHICLE INSPECTION NOTE: The 'add' time allowance as shown in the Labor Time Guide for dealer installed items are included in the amount shown on the vehicle invoice and should not be added to the invoice time.

#### REQUEST FOR REVIEW - TRUCK

VEHICLE SERIES OPERATION DESCRIPTION OPERATION G C K G M S S R V --------------------- NUMBER VIN CODE ------ W C K G M S T R DV --------------------------

STRIP AND/OR RETAINER, FRONT DOOR WINDOW INNER SEALING - R&R OR REPLACE NOTE: Applicable model years: 1987-1988 RIGHT C0120 .4 .4 LEFT C0121 .4 .4

STRAP (HANDLE) AND/OR ESCUTCHEON, ASSIST - R&R OR REPLACE NOTE: Applicable model year: 1988 RIGHT FRONT C3904 .2 .2

MOTOR AND/OR FAN, BLOWER - R&R OR REPLACE NOTE: Applicable model year: 1988

A/C D1322 EXC DIESEL .5 .5 DIESEL 1.9 1.9

CORE EVAPORATOR - REPLACE NOTE: Applicable model year: 1988 FRONT UNIT D3344 2.0 2.0

CARRIER COMPONENTS, SWING-OUT SPARE TIRE - REPLACE NOTE: Applicable model years: 1985-1988

FRAME ASSEMBLY E0590 .6 .6 HINGES AND/OR BUSHINGS E0592 .6 .6 HANDLE AND LATCH E0594 .2 .2 STRIKER PLATE E0596 .2 .2

SENSOR, TRANSMISSION SPEED - REPLACE K2050 .5 .5 NOTE: Applicable model year: 1988 INCLUDES: All manual transmissions.

SENSOR, TRANSMISSION SPEED - REPLACE K6310 .5 .5 NOTE: Applicable model year: 1988 INCLUDES: All automatic transmissions.

MODULE, PULSE WIPER CONTROL - REPLACE N3570 .3 .3 NOTE: Applicable model year: 1988

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.