CLUTCH SHUDDER LAUNCH OR REVERSE. Geo Sprint 1985

For 1990-2009 cars

# CLUTCH SHUDDER LAUNCH OR REVERSE

#### Model and Year 1985 SPRINT

#### TO: ALL CHEVROLET DEALERS

Some early 1985 "M" cars with manual transmissions may exhibit an objec- tionable driveline disturbance due to clutch shudder. The shudder usually occurs during vehicle launch in first or reverse gear and is most notice- able on steep grades.

This shudder condition can be corrected by installing the following applic- able replacement parts on vehicles built prior to the designated V.I.N.'s.

Replace if V.I.N. Part Description Part Number Is Prior To: ---------------- ----------- ------------ Front Engine Mount 96054436 718398

Rear Engine Mount 96051607 703133

Drive Axles Right 96053768 703024 Left 96053769

Use applicable Labor Time and Operation Number.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.