IDLE MICRO SWITCH CORRECTION TO ADJUSTMENT. Geo Sprint 1987

For 1990-2009 cars

# IDLE MICRO SWITCH CORRECTION TO ADJUSTMENT

#### Model and Year: 1985-87 SPRINT SERVICE MANUAL

This bulletin is being issued to correct the adjustment procedure for the Idle Micro Switch shown in Section 6E of the 1985, 1986 and 1987 Sprint Service Manual.

In step number 4 we state "Bend lever down when engine RPM is below specification and up when over specification."

The correct procedure is: "Bend lever up when engine RPM is below specification and down when over specification.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.