SERVICE MANUAL UPDATE SEC. 3B2 MAN. STG. PINION BEARING PLUG. Geo Sprint 1991

For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 3B2 MAN. STG. PINION BEARING PLUG

#### Subject: MANUAL STEERING PINION BEARING PLUG REMOVAL AND INSTALLATION

#### Model and Year: 1989-91 GEO METRO

This bulletin amends service information found in Manual Steering Gear Section 3B2 of the 1989, 1990 and 1991 Geo Metro Service Manual

The J 14859 pinion bearing plug socket has been replaced by the J 39534 pinion bearing plug socket. Use the J 39534 to remove and install the pinion bearing plug on the manual rack and pinion steering gear assembly (Figure 1).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.