SERVICE MANUAL UPDATE-SEC. 7B CHANGE IN M/T FLUID P/N. Geo Storm 1990

For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 7B CHANGE IN M/T FLUID P/N

#### subject: MANUAL TRANSAXLE FLUID

#### Model and Year: 1990 GEO STORM

#### TO: ALL CHEVROLET DEALERS

This bulletin amends the "Checking Transaxle Fluid Level" on page 7B-2 of the 1990 GEO Storm Service Manual (ST371-90).

If manual transaxle fluid needs to be added to the transaxle, add GM #12345349 STF Manual Transaxle Fluid through the filler plug hole. Add fluid until the level reaches the lower lip of the filler plug hole.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.