SERVICE MANUAL UPDATE-SEC. 6D3 GENERATOR UNIT REPAIR. Geo Storm 1992

For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 6D3 GENERATOR UNIT REPAIR

#### Subject: GENERATOR UNIT REPAIR

#### Model and Year: 1992-93 GEO STORM WITH 1.6L ENGINE

This bulletin cancels and supersedes the VIN 6 generator "Unit Repair" procedure on Page 6D3-4 of the 1992 Geo Storm Service Manual (ST371-92) and the "Disassembly, Test and Reassembly - VIN 6" procedure on Page 6D3-5 of the 1993 Geo Storm Service Manual (ST371-93). The generator on a 1992 or 1993 Geo Storm equipped with a VIN 6 engine is now serviceable. Whenever service is required to a 1992 Geo Storm equipped with a VIN 6 engine, use the "Generator - VIN 8" procedure on Page 6D3-6 of the 1992 Geo Storm Service Manual (ST371-92). Whenever service is required to a 1993 Geo Storm equipped with a VIN 6 engine, use the "Disassembly, Test and Reassembly - VIN 8" procedure on Page 6D3- 7 of the 1993 Geo Storm Service Manual (ST371-93).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.