Forward Band Servo Piston Adjustment. Geo Tracker - 4WD 1997

For 1990-2009 cars

1. Hold the servo piston adjusting sleeve (158) with a wrench.
2. Loosen the adjusting sleeve lock nut (165). Be certain the lock nut remains loose.

Tighten
Tighten the adjusting screw (164) to 4.5 N·m (40 lb in).

Refer to Fastener Notice .

3. Loosen the adjusting screw (164) five turns, exactly.
4. Hold the adjusting sleeve and the adjusting screw while tightening the lock nut.

Tighten
Tighten the lock nut (165) to 18.9 N·m (14 lb ft).