Filler Tube Replacement. Geo Tracker - 2WD 1997

For 1990-2009 cars

#### Tools Required

J 36850 Transjel® Transmission Assembly Lubricant

### Removal Procedure

1. Raise the vehicle. Support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove one bolt and the fluid filler tube from the transmission case.
3. Inspect the fluid filler tube O-ring for cuts or other damage. Replace as necessary.

### Installation Procedure

1. Apply J 36850 to the fluid filler tube O-ring.
2. Install the filler tube into the transmission case.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Secure the filler tube with one bolt.

Tighten
Tighten the fluid filler tube bracket bolt to 23 N·m (17 lb ft).

4. Lower the vehicle.