SMU - SECTION 6E3-C4 DRIVEABILITY & EMISSIONS. Geo Tracker - 4WD 1995

For 1990-2009 cars

# SMU - SECTION 6E3-C4 DRIVEABILITY & EMISSIONS

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6E3-C4 - DRIVEABILITY AND EMISSIONS - REVISED FIRING ORDER 1.6 (VIN 6) GRAPHIC ART

#### MODELS: 1995-97 CHEVROLET GEO TRACKER WITH 1.6L ENGINE (VIN 6 - RPO LO1)

THIS BULLETIN IS BEING ISSUED TO REVISE THE FIRING ORDER 1.6L (VIN 6) GRAPHIC ART FOUND IN THE SERVICE MANUAL SECTION, DRIVEABILITY AND EMISSIONS 6E3, SUBSECTION IGNITION SYSTEM C4. THE PURPOSE OF THIS BULLETIN IS TO SHOW THE CORRECT ROTATION OF THE DISTRIBUTOR SHAFT. THE CORRECT ROTATION IS IN A COUNTERCLOCKWISE DIRECTION. THE ATTACHED REPLACEMENT ART SUPERSEDES THE ART ORIGINALLY PUBLISHED IN THE SERVICE MANUAL.

FIGURES: 01 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.