A/T REMOVAL PROCEDURE SERVICE MANUAL UPDATE. Geo Tracker - 4WD 1989

For 1990-2009 cars

# A/T REMOVAL PROCEDURE SERVICE MANUAL UPDATE

#### Model and Year: 1989 GEO TRACKER

#### TO: ALL CHEVROLET DEALERS

The following procedure for removing the automatic transaxle was not included in Section 7A of the 1989 Geo Tracker Service Manual (ST377-89).

#### TRANSMISSION ASSEMBLY

#### Remove or Disconnect

1. Negative battery cable. 2. Detent cable at throttle body unit. 3. Fluid level indicator. 4. Modulator vacuum hose at manifold. 5. Starter. 6. Two upper transmission retaining bolts. 7. Fan shroud bolts. 8. Distributor cap.

#### Important

---------

Support engine from falling back and damaging distributor unit.

9. Interior console. 10. Transfer case shifter, boot assembly. 11. Raise vehicle. 12. Front and rear drive shafts. - Mark drive shaft alignment. 13. Transfer case skid plate. 14. Speedometer cable from transfer case. 15. Flywheel inspection cover. - Mark flywheel and torque converter for re-assembly. 16 Torque converter to flywheel bolts. 17. Shifter linkage. - Shifter cable retaining clip and disconnect cable. 18. Oil cooler lines. 19. Exhaust bracket at catalytic converter and at transmission. 20. Support transmission. 21. Crossmember. 22. Two transmission lower retaining nuts. 23. Lower transrnission and disconnect breather and electrical leads. 24. Transmission and transfer case assembly from vehicle.

#### Install or Connect

1. Transmission and transfer case assembly into vehicle. 2. Breather and electrical leads. 3. Two transmission lower retaining nuts 84 N-m (62 lb. ft.). 4. Crossmember. 5. Speedometer cable to transfer case. 6. Exhaust bracket at catalytic converter and at transmission. 7. Oil cooler lines. 8. Shifter linkage and cable retaining clip. 9. Torque converter to flywheel bolts 50 N-m (37 lb. ft.). 10. Flywheel inspection cover. 11. Front and rear drive shafts 50 N-m (37 lb. ft.). 12. Transfer case skid plate. 13. Lower vehicle. 14. Transfer case shifter and boot assembly. 15. Interior console. 16. Distributor cap. 17. Fan shroud bolts. 18. Two upper transmission retaining bolts 84 N-m (62 lb. ft.). 19. Starter. 20. Modulator vacuum hose at manifold. 21. Fluid level indicator. 22. Detent cable at throttle body unit. 23. Negative battery cable.

#### Adjust

- Shift linkage. - Kick down cable. - Fluid level.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.