SERVICE MANUAL UPDATE CAMBER AND CASTER SPEC.. Geo Tracker - 4WD 1989

For 1990-2009 cars

# SERVICE MANUAL UPDATE CAMBER AND CASTER SPEC.

#### VEHICLES AFFECTED: 1989 TRACKER

SERVICE MANUAL UPDATE

This bulletin is being written to correct the Camber and Caster specification print on page 3A-2 of the 1989 Tracker Service Manual.

The correct specifications are shown below:

Camber .5 degrees +/- 1 degree

Caster 1.5 degrees +/- 1 degree

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.