Clutch Cable Replacement. Geo Tracker - 4WD 1997

For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Loosen the clutch cable adjustment nuts A (3) and B (4).
3. Remove one nut (6) and the clutch cable (5) from the release lever (7) and the clutch cable bracket (2).
4. Remove the clutch cable (5) from the two clutch cable clamps below the radiator.
5. Lower the vehicle.
6. Remove the clutch cable (1) from the upper clutch cable clamp (2) at the left front strut (3).
7. Remove the clutch cable clevis (3) from the clutch pedal shaft arm (2).
8. Remove the two clutch cable grommet bolts (1) and the clutch cable (3) from the vehicle from the engine compartment side of the bulkhead.
9. Inspect the clutch cable (1) for fraying or kinks. Replace as necessary.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the clutch cable (3) into the bulkhead from the engine compartment side; secure with two clutch cable grommet bolts (1).

Tighten
Tighten the clutch cable grommet bolts to 8 N·m (70 lb in).

2. Install the clutch cable clevis (3) to the clutch pedal shaft arm (2).
3. Install the clutch cable (1) into the upper clutch cable clamp (2) at the left front strut tower.
4. Raise and support vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
5. Install the clutch cable (1) into the two clutch cable clamps (2) below the radiator.
6. Install the clutch cable (5) into the clutch release lever (7) and the clutch cable bracket (2); secure with the clutch release lever adjustment nut.
7. Lower the vehicle.
8. For clutch cable adjustment procedures, refer to Clutch Pedal Replacement for clutch pedal height adjustment and Clutch Pedal Free Travel Adjustment .