Reverse Clutch Parts Removal. Geo Tracker - 2WD 1997

For 1990-2009 cars

1. Remove the wave plate (232).

Important: If the clutch plates are not being replaced, they must be installed in their original position.

2. Remove the reverse clutch plates (233) and (234).
3. Remove the reverse clutch pressure plate (236).
4. Inspect the reverse clutch Composition plates (234) for damaged tangs, delamination and excessive wear.
5. Inspect the steel plates (233) for worn lugs and heat damage.