Reverse Clutch Assemble. Geo Tracker - 4WD 1997

For 1990-2009 cars

### Tools Required

J 23327 Third Clutch Spring Compressor

1. Install the reverse clutch piston inner and outer seals (226, 227).
2. Install the reverse clutch piston (228) onto the rear face of the transmission oil pump assembly (222).
3. Install the reverse clutch piston return springs (229).
4. Install the spring seat (230).
5. Install J 23327 .
6. Compress the reverse clutch piston return springs (229).
7. Install the reverse clutch piston return spring seat retainer ring (231).
8. Remove J 23327 .