Transmission General Specifications. Geo Tracker - 2WD 1997

For 1990-2009 cars

Name | Hydra-matic 3L30
--- | ---
Production Location | Strasbourg, France
Vehicle Platform (Engine/Transmission) Usage | E,J Truck
Transmission Drive | Longitudinal Mounted Rear Wheel Drive
Maximum Engine Torque | 300 N·m 221 lb ft
1st Gear Ratio | 2.40:1
2nd Gear Ratio | 1.48:1
3rd Gear Ratio | 1.000:1
Reverse | 2.00:1
Maximum Shift Speed | 6,500 rpm
Torque Converter Size (Diameter of Torque Converter Turbine) | 245 mm
Pressure Taps | Line Pressure
Transmission Fluid Type | Dexron™ III
Transmission Fluid Capacity (Approximate) | Dry: 6 L (6.3 qts)
Transmission Type: 3 | Three Forward Gears
Transmission Type: L | Longitudinal Mount
Product Series | 30
Position Quadrant | P, R, N, D, 2, 1
Case Material | Die Cast Aluminum
Transmission Weight Dry | 53.3 kg (117.5 lbs)
Transmission Weight Wet | 58.6 kg (129.08 lbs)
Maximum Gross Vehicle Weight (GVW) | 3500 kg (7,716 lbs)

Application | Specification
--- | ---
Metric | English
Transmission Fluid Capacities: Pan Removal (Approximate) | 2.9 L | 3.1qts
Transmission Fluid Capacities: Overhaul (Approximate) | 6.0 L | 6.3 qts
Transmission Fluid Type | Dextron® lll | Dextron® lll
Transmission Weight: Dry | 53.3 Kg | 117.50 lb
Transmission Weight: With Fluid | 58.6 Kg | 129.08 lb
Converter Size | 245 mm | 9.64 in
6 Position Quadrant | P, R, N,D,2,1 | P,R,N,D,2,1,
Pressure Taps Available | Line Pressure | Line Pressure
Case Materials | Die Cast Aluminum | Die Cast Aluminum