SETTING CLOCK ON ETR AM-FM STEREO WITH SEEK AND SCAN. Geo Tracker - 4WD 1990

For 1990-2009 cars

# SETTING CLOCK ON ETR AM-FM STEREO WITH SEEK AND SCAN

#### Model and Year: 1990 M, R CARS AND J TRUCK (TRACKER)

The directions for the ETR AM-FM Stereo with Seek and Scan described in Section 2C of the Owner's Manual do not apply. The proper operating procedures for the entire system are as follows:

ETR AM-FM STERO (SEEK/SCAN)

TO PLAY THE RADIO

Push the power knob PWR/VOL to turn radio on; push again to turn off. (It also goes off with ignition key.)

ADJUST VOLUME - The same knob adjusts the volume; turn right for more volume.

AM/FM SELECTION - Press AM/FM to receive AM or FM (the lighted display shows your selection momentarily).

SEEK - Press SEEK UP to go to the next station and stay there. (It will find another station each time you press it.) DOWN SEEK finds the next lower station.

SCAN - Press SCAN to sample each station for about five seconds; press again to stop and listen to something you like. NOTE: The display flash frequency and band during SCAN.

MANUAL TUNING - Press TUNE UP and hold to tune manually. (Radio tunes as long as pushbutton is held.) Press DOWN TUNE to tune down the band.

PUSHBUTTONS - There are five pushbuttons numbered 1 through 5. They help you return to your favorite stations. Set the pushbuttons as follows:

- Tune in the station you want. - Press and hold one of the pushbuttons for longer than 2 seconds. - NOTE: Audio mutes and then returns when the station is stored.

SETTING CLOCK - Press RCL and hold (with time showing on the display) and within five seconds, press DOWN TUNE until clock shows correct hours. Press and hold TUNE UP until clock shows correct minutes.

RECALL - Press RCL to switch between time and frequency on the display.

DISPLAY PRIORITY - You may change display priority from time to frequency by pressing and holding RCL and within one second pressing SEEK UP. Repeat to change back.

STEREO - Stereo is received by tuning to any FM station broadcasting in stereo (ST is displayed in the graphic display).

TO ADJUST TONE - Rotate the TONE control clockwise to increase treble; counterclock- wise rotation favors the bass. A detent gives the center of rotation.

TO ADJUST SPEAKER - Turn FADE control (located behind the TONE knob) clockwise to favor the rear speakers. A detent gives the center of rotation.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.