SERVICE MANUAL UPDATE DIFFERENTIAL BEARING CAP BOLTS. Geo Tracker - 4WD 1989

For 1990-2009 cars

# SERVICE MANUAL UPDATE DIFFERENTIAL BEARING CAP BOLTS

#### Model and Year: 1989 GEO TRACKER SERVICE MANUAL (ST377-89)

This bulletin is being written to correct the front and rear differential bearing cap torque printed on page 4D-14 of the 1989 GEO Tracker Service manual. The torque values printed below should be used when tightening front and rear differential bearing caps:

Front Differential Bearing Cap (60 N.m) 44 lb. ft.

Rear Differential Bearing Cap (85 N.m) 63 lb. ft.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.