WARRANTY ADMIN. CHEVROLET QUALITY APPROVED CONVERTER. Geo Tracker - 4WD 1996

For 1990-2009 cars

# WARRANTY ADMIN. CHEVROLET QUALITY APPROVED CONVERTER

REVISION: 09/16/95

THIS BULLETIN IS BEING REVISED TO INFORM "GM OF CANADA" AND "NAES" DEALERS THAT THEY ARE NOT AUTHORIZED TO UTILIZE THIS SERVICE BULLETIN. **********************************************************************

REVISION: 10/23/95

THIS BULLETIN IS BEING REVISED TO ADD INFORMATION TO THE TEXT. **********************************************************************

#### SUBJECT: WARRANTY ADMINISTRATION - CHEVROLET QUALITY APPROVED CONVERTER PROGRAM (C.Q.A.C.P.) UPFITTED UNITS/SPLIT PDI ALLOWANCE

#### MODEL: 1996 CHEVROLET LIGHT DUTY TRUCKS

#### ATTENTION:

DEALER SERVICE MANAGEMENT AND BUSINESS MANAGER

'GM OF CANADA' AND 'NAES' DEALERS ARE NOT AUTHORIZED TO UTILIZE THIS SERVICE BULLETIN.

THE PURPOSE OF THIS BULLETIN IS TO INFORM RETAIL AND WHOLESALE SERVICE PERSONNEL OF THE SPLIT PDI ALLOWANCE CHANGES FOR THE 1996 MODEL YEAR. THE LISTED TIMES WILL BECOME EFFECTIVE WITH R.O.'S DATED 11/1/95.

AS A REMINDER, C.Q.A.C.P. UPFITTERS, OR THEIR DESIGNATED DEALER, ARE RESPONSIBLE FOR THE MECHANICAL PORTION OF THE PDI, INCLUDING THE ITEMS LISTED UNDER THE FOLLOWING OPERATIONS FROM THE PDI FORM:

**UNDERHOOD** **BODY/CHASSIS** **ROAD TEST** **UNDER VEHICLE**

MECHANICAL PDI ALLOWANCES ARE LISTED BELOW UNDER THE COLUMN "MECHANICAL/BAILMENT."

C.Q.A.C.P. UPFITTERS, OR THEIR DESIGNATED DEALER, ARE ALSO RESPONSIBLE FOR ALL PDI ALLOWANCE ADD-ONS WHICH INCLUDE:

SERIES OPTION ALLOWANCE

C/K/G/P MIRROR, CAMPER (DF2) 0.4 C/K WHEEL COVERS/CENTER CAPS (PO6) 0.1 G WHEEL COVERS/CENTER CAPS N90,N67) 0.1 S/T INSTALL WHEEL AND TIRE ON CARRIER INCLUDING COVER (P16) 0.1 M/L LUGGAGE CARRIER (V54) 0.6 TAHOE 2DR LUGGAGE CARRIER (V54) 0.3 TAHOE 4DR LUGGAGE CARRIER (V54) 0.4 C/K SUBURBAN LUGGAGE CARRIER (V54) 0.6 TAHOE RUNNING BOARDS (BVE) 0.5 SUBURBAN RUNNING BOARDS (BVE) 0.5 C/K/G/P DUAL REAR WHEELS (R05) 0.1 C/K MIRRORS, WEST COAST TYPE (DG5) 0.4 S/T PICKUP LIC. BRKT. (ONLY ON MODELS W/0 REAR BUMPER OPTION (VF6) 0.2

**NOTE: THE SPLIT PDI DOES NOT APPLY TO THE C.Q.A.C.P. ACCOUNTS THAT PRODUCE SCHOOL BUSSES; TYPICALLY ON G/P CUTAWAYS. THESE ACCOUNTS WILL RECEIVE THE FULL PDI ALLOWANCE PAID TO EITHER THE C.Q.A.C.P. UPFITTER OR THEIR DESIGNATED DEALER.**

** INVOICE OPTION CODE "R6P",** SIGNIFIES THAT THIS UPFITTED VEHICLE MAY BE ELIGIBLE FOR THE APPEARANCE PORTION OF THE PDI. CHEVROLET RETAIL DELIVERING DEALERS ARE RESPONSIBLE FOR COMPLETING ALL ITEMS LISTED UNDER THE OPERATION "APPEARANCE" (INCLUDING "AIM HEADLIGHTS-CQACP UNITS ONLY"); LOCATED IN THE LOWER RIGHT HAND PORTION OF THE CHEVROLET PRE-DELIVERY INSPECTION FORM.

CHEVROLET RETAIL DELIVERING DEALERS SHOULD SUBMIT A WARRANTY CLAIM FOR THE APPROPRIATE PDI APPEARANCE ALLOWANCE USING LABOR OPERATION Z7001; APPEARANCE ALLOWANCES ARE FOUND UNDER THE COLUMN "APPEARANCE/RETAIL."

MECHANICAL/ APPEARANCE/ BAILMENT RETAIL

G-VAN .7 .8 G-CUTAWAY 1.1 .7 H-CUTAWAY 1.1 .7 M-VAN .7 .7 BLAZER .6 .6 C/K PICKUP .7 .6 C/K CHASSIS CAB .7 .6 S-SERIES PICKUP .6 .6 SUBURBAN .7 .7 TAHOE .7 .7 LMV .7 .7 TRACKER .7 .7

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER." THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 CHEVROLET MOTOR DIVISION, GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.