Transfer Case Adapter Seal Replacement. Geo Tracker - 2WD 1996

For 1990-2009 cars

#### Tools Required

• | J 6125-B Slide Hammer

• | J 23129 Converter Housing Seal and Extension Housing Oil Seal Remover

• | J 35538 Adapter Case Seal Installer

• | J 36850 Transjel® Transmission Assembly Lubricant

### Removal Procedure

1. Raise the vehicle. Support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Support the transmission with a suitable hydraulic jack.
3. Remove the transfer case from the vehicle.
4. Remove the transfer adapter case seal (1) from the transfer adapter case using the J 23129 and the J 6125-B .
5. Inspect the transfer adapter case for cracks and other damage. Replace as necessary.

### Installation Procedure

1. Apply a thin coat of J 36850 to the transfer adapter case seal surface.
2. Install the new transfer adapter case seal (1) into the transfer adapter case using a J 35538 .
3. Apply J 36850 to the new transfer adapter case seal lip.
4. Install the transfer case into the vehicle. Refer to Transfer Case Replacement in Driveline/Axle.
5. Remove the hydraulic jack from under the transmission.
6. Lower the vehicle.