For 1990-2009 cars

1. Remove the shift control lever shaft seal by holding onto the seal and hitting the end of the shift control lever with a soft-face hammer.
2. Remove the control lever boot.
3. Remove the shift control shaft boot from the shift control lever retainer.
4. Remove the shift control lever retainer bolts.
5. Remove the shift control lever retainer.
6. Remove the control lever housing gasket.
7. Remove the shift control lever assembly from the shift control housing.

Do not remove the shift lever seat or bushing from the lever. The shift lever seat and bushing can only be serviced with the lever.