For 1990-2009 cars

#### Special Tools

• | EN-48034 Crankshaft Balancer Installer

• | J 45059 Angle Meter

For equivalent regional tools, refer to Special Tools

1. Install the crankshaft balancer using EN-48034 installer .
2. Remove EN-48034 installer .
3. Hold the flywheel or back of the crankshaft. The crankshaft balancer does not have a keyway so the crankshaft could turn when tightening, causing an improper torque.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the crankshaft balancer washer and new bolt.

4.1. | Tighten the new crankshaft balancer bolt while holding the back to 150 N·m (110 lb ft).

4.2. | Use J 45059 meter to tighten the crankshaft balancer bolt an additional 180 degrees.