For 1990-2009 cars

#### Tools Required

J 44219 Housing Alignment Pins

1. Apply a 3 mm (0.12 in) bead of GM P/N 12378521 (Canadian P/N 88901148) to the rear sealing surface of the block (1).
2. Install J 44219 into the block.

Important: With the help of the plastic installation aid (supplied with the new seal), be sure the lip of the seal faces inward.

3. Slide the crankshaft rear oil seal housing and bolts over the alignment pins J 44219 and crankshaft, except the 2 in place of the guide pins.
4. Remove J 44219 .
5. Snug the crankshaft rear oil seal housing bolts.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

6. Install the remaining two crankshaft rear oil seal housing bolts.

Tighten
Tighten the crankshaft rear oil seal housing bolts to 10 N·m (89 lb in).

7. Wipe off any excess material from the bottom of the oil pan sealing area (1).