For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Adjuster Plug - Allen Head

- First Pass

15 N·m

11 lb ft

- Final Pass

25 Degrees Back

Adjuster Plug - Hex Head

- First Pass

12 N·m

106 lb in

- Final Pass

105 Degrees Back

Adjuster Plug Lock Nut | 60 N·m | 44 lb ft
Engine Wiring Harness Bracket Bolt (LH8) | 40 N·m | 30 lb ft
Cylinder Pipe Fittings Cylinder End | 15 N·m | 11 lb ft
Generator Bracket Bolt (LH8) | 50 N·m | 37 lb ft
Inner Tie Rod | 100 N·m | 74 lb ft
Outer Tie Rod Jam Nut | 75 N·m | 55 lb ft
Outer Tie Rod Retaining Nut

- First Pass

45 N·m

33 lb ft

- Final Pass

95 Degrees

Power Steering Fluid Reservoir Bracket Bolt (LH8) | 25 N·m | 18 lb ft
Power Steering Gear Inlet and Outlet Hose Bracket Bolt | 9 N·m | 80 lb in
Power Steering Gear Inlet and Outlet Hose Fitting | 25 N·m | 18 lb ft
Power Steering Gear Inlet and Outlet Hose Retaining Plate Bolt | 12 N·m | 106 lb in
Power Steering Pump Bolt (LH8) | 25 N·m | 18 lb ft
Power Steering Pump Bracket Bolt (LLV, LLR) | 50 N·m | 37 lb ft
Power Steering Pump Flow Control Valve (LLV, LLR) | 75 N·m | 55 lb ft
Power Steering Pump Mounting Bolt (LLV, LLR) | 25 N·m | 18 lb ft
Steering Gear Bolt (isolator clamp bolt) | 100 N·m | 74 lb ft
Steering Gear Bolt (long bolt) | 130 N·m | 96 lb ft
Steering Gear Cylinder Pipe Fitting | 15 N·m | 11 lb ft