For 1990-2009 cars

## Folding Seat Replacement Extended Cab

### Removal Procedure

1. Remove the 2 bolts securing the folding rear seat cushion assembly to the vehicle.
2. Remove the rear seat from the vehicle.

### Installation Procedure

1. Position the folding rear seat cushion assembly in the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the 2 bolts securing the folding rear seat cushion assembly to the vehicle.

Tighten
Tighten the folding rear seat cushion assembly bolts to 52.5 N·m (39 lb ft).