For 1990-2009 cars

## Body Side Lower Rear Molding Replacement B84

Callout | Component Name
--- | ---
1 | Body Side Lower Rear Molding Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. The part and surface should be 21°C (70°F) prior to installation. The vehicle should remain 21°C (70°F) for one hour after assembly to allow adhesive to develop sufficient bond strength.
2. Use a J 25070 Heat Gun to remove the rear body side lower molding.
3. When removing protective liners from adhesive tape, be careful not to touch tape with hands and do not allow tape to come in contact with dirt or any foreign matter prior to adhesion.
4. Clean all the adhesive from the cab side, wipe the surface dry with a clean lint-free towel prior to installing new rear body side lower molding.
5. Ensure to close the door prior to attaching the new molding to the rear body side cab.
6. Peel the protective liner from the adhesive tape and secure the rear body side cab molding.
7. Using a towel and hand pressure, wet out the entire length of the molding starting at the rear edge working forward.