For 1990-2009 cars

### Removal Procedure

1. Remove the seat from the vehicle. Refer to Split Bench Seat Replacement or Front Seat Replacement - Bucket .
2. Remove the seat back cover and pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .
3. Remove the lumbar assembly. Refer to Front Seat Lumbar Support Replacement .
4. Remove the 4 seat recliner mounting bolts (1) securing the seat back frame to the seat back recliner mechanism.
5. Remove the seat back frame.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat back frame to the seat back recliner mechanism with 4 bolts (1).

Tighten
Tighten the front seat recliner bolts to 24 N·m (18 lb ft).

2. Install the lumbar assembly. Refer to Front Seat Lumbar Support Replacement .
3. Install the seat back pad and cover. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .
4. Install the seat in the vehicle. Refer to Split Bench Seat Replacement or Front Seat Replacement - Bucket .