For 1990-2009 cars

### Removal Procedure

1. Remove the tilt spring. Refer to Steering Column Tilt Spring Replacement .
2. Remove the tilt lever bolt.
3. Remove the tilt lever.

### Installation Procedure

1. Align the tilt lever in the steering column.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the tilt lever bolt.

Tighten
Tighten the bolt to 1 N·m (9 lb in).

3. Install the tilt spring. Refer to Steering Column Tilt Spring Replacement .