For 1990-2009 cars

### Removal Procedure

1. Remove the seat cushion outer trim panel. Refer to Seat Cushion Outer Trim Panel Replacement .
2. Remove the switch bezel from the seat assembly. Refer to Driver Seat and Passenger Seat Adjuster Switch Bezel Replacement .
3. Remove the buttons from the switch (2).
4. Release the tabs (1) that retain the seat switch (2) to the seat bezel.
5. Disconnect the power seat switch harness (1) from the seat harness.
6. Remove the power seat switch from the seat bezel.

### Installation Procedure

1. Connect the power seat switch harness (1) to the seat harness.
2. Install the power seat switch (2) to the seat bezel. Verify that the retaining tabs (1) are fully seated.
3. Install the buttons on the switch.
4. Install the switch bezel assembly to the seat assembly. Refer to Driver Seat and Passenger Seat Adjuster Switch Bezel Replacement .
5. Install the seat cushion outer trim panel. Refer to Seat Cushion Outer Trim Panel Replacement .