For 1990-2009 cars

### Removal Procedure

Caution: Refer to Brake Dust Caution in the Preface section.

Notice: Refer to Brake Caliper Notice in the Preface section.

1. Remove the front brake caliper. Refer to Brake Caliper Replacement .
2. Remove the brake pads from the mounting bracket.
3. Remove the mounting bolts for the brake caliper mounting bracket.
4. Remove the brake caliper mounting bracket.

### Installation Procedure

1. Position the mounting bracket on the steering knuckle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the mounting bolts bracket.

Tighten
Tighten the mounting bolts to 175 N·m (129 lb ft).

3. Install the brake pads in the mounting bracket.
4. Install the brake caliper. Refer to Brake Caliper Replacement .