For 1990-2009 cars

### Removal Procedure

1. Remove the left front door sill trim plate. Refer to Front Side Door Sill Plate Replacement .
2. Grasp the left hinge pillar trim panel and gently pull the panel away from the body to release the fasteners.
3. Remove any fasteners that may have pulled away from the panel and reinstall them to the back of the panel.
4. Slide the panel forward so the panel unhooks from around the front door frame.
5. Remove the left hinge pillar trim panel from the vehicle.

### Installation Procedure

1. Position the left hinge pillar trim panel over the pillar and door sill.
2. Ensure that the panel fasteners are aligned with the holes in the body.
3. Install the panel by pushing firmly against the body to seat the panel fasteners.
4. Install the left front door sill trim plate. Refer to Front Side Door Sill Plate Replacement .