For 1990-2009 cars

### Removal Procedure

1. Disconnect the accelerator pedal position (APP) sensor electrical connector.
2. Remove the APP sensor nuts.
3. Remove the APP sensor from the vehicle.

### Installation Procedure

1. Position the APP sensor over the studs.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the APP sensor nuts.

Tighten
Tighten the APP sensor mounting nuts to 9 N·m (80 lb in).

3. Connect the APP sensor electrical connector.
4. Inspect below the pedal for binding, to ensure full range of motion.