For 1990-2009 cars

### Removal Procedure

1. Remove the seat from the vehicle. Refer to Front Seat Replacement - Bucket or Split Bench Seat Replacement .
2. Disconnect the seat belt buckle electrical connector (1).
3. Remove the bolt (2) securing the seat belt buckle assembly (1) to the seat adjuster.
4. Pull the seat belt buckle assembly (1) out though the opening in the seat cushion.

### Installation Procedure

1. Install the seat belt buckle assembly (1) through the seat cushion pad.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the seat belt buckle assembly (1) to the seat adjuster with the bolt (2).

Tighten
Tighten the front seat belt buckle bolt to 55 N·m (41 lb ft).

3. Connect the seat belt buckle electrical connector (1).
4. Install the seat from the vehicle. Refer to Front Seat Replacement - Bucket or Split Bench Seat Replacement .