For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Power Steering System General Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Power Steering System
2 | Verify that power steering fluid leaks are present. Is the power steering system leaking? | Go to Step 3 | System OK
3 | Inspect the power steering system fittings. Are the fittings leaking? | Go to Step 7 | Go to Step 4
4 | Inspect the power steering hoses. Are the hoses leaking? | Go to Step 8 | Go to Step 5
5 | Inspect the power steering pump and the reservoir for leaks. Is the power steering pump or reservoir leaking? | Go to Step 9 | Go to Step 6
6 | Inspect the power steering gear for leaks. Is the power steering gear leaking? | Go to Step 10 | --
7 | Tighten the fittings. Refer to Fastener Tightening Specifications. Did you complete the repair? | Go to Step 11 | --
8 | Replace the power steering hoses. Refer to Power Steering Gear Inlet and Outlet Hose Replacement. Did you complete the repair? | Go to Step 11 | --
9 | Replace the power steering pump. Refer to Power Steering Pump Replacement. Did you complete the repair? | Go to Step 11 | --
10 | Replace the power steering gear. Refer to Steering Gear Replacement. Did you complete the repair? | Go to Step 11 | --
11 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3