For 1990-2009 cars

### Removal Procedure

1. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the rear door inside handle. Refer to Rear Side Door Inside Handle Replacement .
3. Remove the rear door speaker. Refer to Radio Rear Side Door Speaker Replacement.
4. Remove the rear door water deflector from the rear door inner panel.
5. Pull the electrical connectors through the slit in the water deflector.

### Installation Procedure

1. Align the rear door water deflector to the rear door inner panel. Secure the water deflector at the corners.
2. Pull the rear door electrical connectors through the slit in the water deflector.
3. Install the rear door water deflector. Start pressing the adhesive pattern at the bottom center and working outward and upward in order to prevent puckering.
4. Install the rear door speaker. Refer to Radio Rear Side Door Speaker Replacement.
5. Install the rear door inside handle. Refer to Rear Side Door Inside Handle Replacement .
6. Install the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .